MAX 3000A devices are low cost, high performance devices based on the Altera MAX architecture. The EEPROM-based MAX 3000A devices operate with a 3.3-V supply voltage and provide 600 to 10,000 usable gates and counter speeds of up to 227.3 MHz. 