MAX 7000B devices are high-density, high performance devices based on Altera’s second generation MAX architecture. The EEPROM-based devices operate with a 2.5-V supply voltage and provide 600 to 10,000 usable gates and counter speeds up to 303.0 MHz.