The MAX 7000 family of high-density, high performance PLDs is based on Altera’s second generation MAX architecture. The EEPROM-based MAX 7000 family provides 600 to 5,000 usable gates and counter speeds of up to 175.4 MHz.