MAX2 devices are low-cost CPLDs containing low power process technology, delivering twice the performance of previous MAX devices. With an on-chip regulator accepting 1.8-3.3V of power supply, it can support clock frequencies of up to 300 MHz