The Lattice MachXO family combines CPLD and FPGA attributes to provide an optimal solution for control-type applications. It includes PLLs and embedded memory, along with CPLD features you would normally expect like instant-on, non-volatility and security.